**<MKSID-5088>**



core Flight System (cFS) File Manager (FM) Application

Requirements Document

Version 1.5

**January 25, 2017**

<MKSID-5091>

1.0       Introduction

1.1        Document Purpose

The core Flight Software System (cFS) File Manager Application will be developed by the Flight Software Branch (FSB) of the Software Engineering Division (SED).  The purpose of this requirements specification is to define the requirements to be satisfied by the File Manager Application.

This application is developed for re-use.  For this reason, several nomenclatures are used in this document to identify configurations for a mission.  The cFS is specified as a multi-platform product. Mission-specific features and customization requirements which are applicable for all platforms are tagged with <MISSION\_DEFINED>.  Platform-specific features and customizations requirements are tagged with either “<PLATFORM\_DEFINED>” or “<OPTIONAL>.”  Additional nomenclature is used along with the tag to specify a cFS default value for the platform-specific feature: “<PLATFORM\_DEFINED, Default\_Value>”.  Reference platforms (single processor and multi-processor architectures) are defined to supply the default cFS application configuration.  These configurations define the “maximum” cFS Application deployments such that any refined deployment is a subset of a reference platform. 

1.2        Document Scope

The scope of this document is limited to the specification of requirements for the File Manager software requirements.  These include functional, performance, qualification, and design requirements.

1.3        Document Organization

This document is organized into three additional sections and several appendices.

Section 2 gives the File Manager context.

Section 3 documents the File Manager system design decisions and constraints.

Section 4 contains the File Manager high level functional and performance requirements.

Section 5 contains the File Manager detailed functional and performance requirements.


1.4        Relevant Documents

1.4.1     Parent Documents

cFS File Manager Application Heritage Analysis 582-2007-011  
   
1.4.2     Reference Documents

Operating System Abstraction Layer (OSAL) Library API   
cFE Application Developer’s Guide  582-2007-001  
cFE User’s Guide

2.0       **cFS File Manager Application Context**

  
The cFS File Manager (FM) application provides a ground interface for managing onboard file systems.  The application file management services  to the ground include copying files, moving or renaming files, deleting files, decompressing files, concatenating files,  retrieving file and directory status information, creating directories, removing directories, and retrieving directory listings.   
   
The cFS FM context shows use of a complete cFS, presenting interfaces with other cFS applications.  SCH is the cFS scheduler application that submits periodic housekeeping requests to FM. Commands come from the cFS Command Ingest application (CI). Event messages and housekeeping packets are routed to the appropriate cFS output application, the Housekeeping (HK), Telemetry Output (TO), and/or Data Storage (DS) application.  All accesses to the file system(s) are through the OS API layer of the cFE.    
   
File systems can exist on RAM and EEPROM as well as custom devices such as a Solid State Recorder (SRR).  The OSAL provides the interface to the file systems on any available devices.  Custom devices such as SSRs will be handled outside of FM (potentially by another application).  
   
   
 

**Figure 1.0** – cFS FM Context

2.1        Assumptions

The following list summarizes the assumptions made by the cFS File Manager Application:

* cFE and OSAL are being used
* All FM operations apply to file systems only (no ground-to-flight or flight-to-ground operations.  Those are handled by a File Transfer Application such as CFDP.
* cFE provides the capability to specify the default CRC algorithm to use.  This gives FM the flexibility to use mission specified CRC required.

3.0       Design Specifications

The File Manager Application’s requirements and design are based on the results of the cFS heritage analysis effort.  The results of the heritage analysis are documented in the cFS File Manager Application Heritage Analysis document.  
   
The File Manager Application is based on the Core Flight Executive (cFE) and the OSAL. In addition, FM exists in the context of the cFS architecture  
   
   
4.0       Subsystem Requirements

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| ID | ReqID | Text | Rational | Heritage Reference |
| 5456 | cFS-200 | The cFS shall provide file/directory management commands for the on-board file system. | Ground must be able to manage the on-board file systems. | LRO |

<MKSID-5339>

5.0       Detailed Requirements

The following are the detailed requirements for File Manager.  All files must be fully-qualified (i.e. full path specified).  In order to distinguish between requirements that require a filename as a parameter from those that just require a directory, the following convention is used:

* command-specified file – denotes that a fully qualified filename must be used (i.e. full path including device name, directory path and filename)
* command-specified directory – denotes that only the device and directory path  is specified.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| ID | ReqID | Text | Rational | Heritage Reference |
|  |  | 5.1        Basic Command Requirements |  |  |
| 5464 | FM1000 | Upon receipt of a No-Op command, FM shall increment the Valid Command Counter and generate an event message. | Debug command to verify application is alive | LRO, BAT, JWST |
| 5466 | FM1001 | Upon receipt of a Reset Counters command,  FM shall reset the following housekeeping variables to a value of zero:           a) Valid Command Counter         b) Command Rejected Counter | Important for testing and on-orbit in order to start with a “clean slate” | LRO, BAT, JWST |
| 5472 | FM1002 | If the computed length of any FM command is not equal to the length contained in the message header, FM shall reject the command | Basic command verification in the event of  SEU or memory corruption | LRO, BAT, JWST |
| 5474 | FM1003 | If FM accepts any command as valid, FM shall execute the command, increment the FM Valid Command  Counter and issue an event message | Operators require positive feedback from successful commands | LRO, BAT, JWST |
| 5476 | FM1004 | If FM rejects any command, FM shall abort the command execution, increment the FM Command Rejected Counter and issue an error event message | Operators require notification of command failures | LRO, BAT, JWST |
| 5478 | FM1005 | If the filename specified in any FM command is not valid, FM shall reject the command | If the filename is not valid then want to reject the command.  non-fully-qualified filenames will be considered invalid | LRO, BAT, JWST |
| 5480 | FM1006 | If the directory specified in any FM command is not valid, FM shall reject the command | If an invalid directory is specified than want to reject the command | LRO, BAT, JWST |
| 5484 | FM1008 | The cFS FM FSW shall utilize full path specifications having a maximum length of <PLATFORM\_DEFINED> characters for all command input arguments requiring a file or pathname. | Fully qualified filenames or paths help ensure the correct files/directories are being manipulated.  This requirement is intended to prevent “assumed” pathnames from being used by cFS FM. | LRO, BAT, JWST |
| 5486 | FM1009 | Upon receipt of the Set Table Entry State Command, FM will set the enable/disable state for the specified entry in the File System Free Space Table. |  | None |
| 5488 | FM1009.1 | If the File System Free Space table has not been loaded FM will reject the command and send an event message |  | None |
| 5490 | FM1009.2 | If the command-specified entry in the File System Free Space Table is invalid FM will reject the command and send an event message |  | None |
| 5492 | FM1009.3 | If the command-specified state is invalid FM will reject the command and send an event message |  | None |
| 5494 | FM1009.4 | If the command-specified entry in the File System Free Space Table is unused FM will reject the command and send an event message |  | None |
|  |  | 5.2        File Management |  |  |
| 5500 | FM2002 | Upon receipt of a File Copy command, FM shall copy the command-specified file to the command-specified destination file | Copy of a fully-qualified file to another fully-qualified file (copy a file to another directory and rename it) | LRO, BAT, JWST |
| 5502 | |  |  | | --- | --- | | |  | | --- | | FM2002.1 | | | If the command-specified destination file exists and the command-specified overwrite flag is set to FALSE, FM shall reject the command | Want to prevent files from being overwritten.  Users must explicitly request file to be overwritten. |  |
| 5508 | FM2004 | Upon receipt of a Move command, FM shall move the command-specified file to the command-specified destination file. | Creates a new destination file, move the contents of the source file into the destination file, and then delete the source file. | LRO, BAT, JWST |
| 5510 | FM2004.1 | If the command-specified destination file exists and the command-specified overwrite flag is set to FALSE, FM shall reject the command | Want to prevent files from being overwritten.  Users must explicitly request file to be overwritten. |  |
| 5514 | FM2005 | Upon receipt of a Rename command, FM shall rename the command-specified file to the command-specified destination file. | Rename can work faster than move command because the entire contents of the file don't need to be moved, only the name gets changed.  If there happen to be a situation where memory was very low, the move command may not be possible due to the fact that a new source file is created before the old one is deleted. | LRO (as of 11/13/07), BAT, JWST |
| 5516 | FM2005.1 | If the command-specified destination file exists, FM shall reject the command. | Want to prevent files from being overwritten.  Users must delete the file first before performing this operation. |  |
| 5522 | FM2007 | Upon receipt of a Delete All Files command, FM shall delete all the files in the command-specified directory. | Typical delete \*.\* command | LRO, BAT |
| 5524 | FM2007.1 | If the command-specified directory contains an open file, FM shall not delete the open file. | The command was a success, however, want to notify the ground that there were files that were not deleted |  |
| 5526 | FM2007.1.1 | For any open files that are not deleted, FM shall issue one event message. |  |  |
| 5528 | FM2007.2 | If the command-specified directory contains a subdirectory, FM shall not delete the subdirectory. | This requirement protects against accidental deletion of subdirectories.  Operator may want to remove files in directories and subdirectories but leave the directory structure in place.  Operators should use the Delete Directory command in order to delete a directory. |  |
| 5530 | FM2007.2.1 | For any subdirectories are not deleted, FM shall issue one event message. |  |  |
| 5532 | FM2008 | Upon receipt of a Delete command, FM shall delete the command-specified file. | Command file operation | LRO, BAT |
| 5536 | FM2008.1 | If the command-specified file is open, FM shall reject the command to delete the file. |  | LRO, BAT |
| 5538 | |  |  | | --- | --- | | |  | | --- | | FM2008.2 | | | If the command-specified file is a directory, FM shall reject the command. | This requirement protects against accidental deletion of a directory.  Operators should use the Delete Directory command in order to delete a directory. |  |
| 5540 | FM2009 | Upon receipt of a Decompress command, FM shall decompress the command-specified file to the command-specified file. | Need to be able to decompress compressed files.  Full-qualified path must be specified.  Should prevent the case where user tries to uncompress to file of same name? | LRO, JWST |
| 5542 | FM2009.1 | If the command-specified destination file exists, FM shall reject the command. | Want to prevent files from being overwritten.  Users must delete the file first before performing this operation. |  |
| 5544 | FM2010 | Upon receipt of a Concatenate command, FM shall concatenate the command-specified file with the second command-specified file, copying the result to the command-specified destination file. | Concatenates 2 files together, producing a 3rd file.  Assumes fully qualified paths | LRO |
| 5546 | FM2010.1 | If the command-specified destination file exists, FM shall reject the command | Want to prevent files from being overwritten.  Users must delete the file first before performing this operation. |  |
| 5548 | FM2011 | Upon receipt of a File Info command, FM shall generate a message containing the following for the command-specified "file:"   1. the file size 2. last modification time 3. file status (Open, Closed, or Non-existent) 4. <MISSION\_DEFINED> CRC 5. the file mode (permissions), as a 4-byte value 6. command-specified filename | Basic file information | LRO, BAT, JWST |
| 5550 | FM2012 | Upon receipt of a List Open Files command, FM shall generate a message containing:   1. the number of open files 2. Up to <PLATFORM\_DEFINED> names/paths (of each open file) and the application name that has opened the file | Provides operators info about open files -   Files that are open should not be deleted or downlinked.  If too many files are open at once, the system could run slower than expected, or decline another file from being opened.  Note that the <MISSION\_DEFINED> limit is imposed in support of fixed size telemetry messages. | LRO |
| 145948 | FM2013 | Upon receipt of a Set File Permissions command, FM shall set the command-specified file's permissions to the command-specified mode.    Note: The mode is defined as a 4-byte value | Basic file operations. Provides operators with the ability to change the read, write, execute permissions of a file. |  |
|  |  | **5.3        Directory Management** |  |  |
| 5554 | FM3000 | Upon receipt of a Create Directory command, FM shall create the command-specified directory on the command-specified file system. | Create directories and subdirectories on the file system. | LRO, BAT, JWST |
| 5556 | FM3001 | Upon receipt of a Delete command, FM shall remove the command-specified directory from the command-specified file system. |  | LRO, BAT, JWST |
| 5558 | FM3001.1 | If the specified directory contains at least one file or subdirectory, the command shall be rejected | Require operators to explicitly remove all files before deleting the directory.  Protection against accidentally deleting of a non-empty directory. | LRO, BAT, JWST |
| 5560 | FM3002 | Upon receipt of a Directory Listing To File command, FM shall write the contents of the command-specified directory on any of the on-board file systems to the command-specified file. The following shall be written:   1. Directory name 2. file size in bytes of each file 3. last modification time of each file 4. Filename of each file 5. Mode (permissions), as a 4-byte value, of each file | Get a directory listing and pipe it to a file for downlink.  Note that the modification time format is specified by a cFE configuration parameter (TAI or UTC) | LRO, BAT, JWST |
| 5562 | FM3002.1 | FM shall issue an event message that reports:   1. The number of filenames written to the specified file 2. The total number of files in the directory 3. The command-specified file’s filename |  | LRO, BAT, JWST |
| 5564 | FM3002.2 | FM shall use the <PLATFORM\_DEFINED> default filename if a file is not specified | cFS standard.  Want to provide flexibility to either use the same filename every time you get a directory listing or specify a new filename. |  |
| 145989 | FM3002.3 | If the command-specified GetSizeTimeMode flag is set to FALSE, FM shall initialize following values to Zero:   1. file size in bytes of each file 2. last modification time of each file 3. Mode (permissions), as a 4-byte value, of each file     Note: the lettering of the listed values is kept in sync with parent requirement | Obtaining file size, time, and permissions may be CPU intensive | GPM, NICER |
| 5566 | FM3003 | Upon receipt of a Directory Listing command, FM shall generate a message containing the following for up to <PLATFORM\_DEFINED> consecutive files starting at the command specified offset:   1. Directory name 2. file size in bytes of each file 3. last modification time of each file 4. Filename of each file 5. Mode (permissions), as a 4-byte value, of each file | Similar to FM3002 command, however, the directory listing is output in a message instead of a file.  May make it easier for the ground to view (one step process). In addition, if there is a problem with the file system, writing to a file (as FM3002 does) is not reliable. The command specified offset is used since there is a maximum number of files that can be downlinked (offset into the file list).  Note that the modification time format is specified by a cFE configuration parameter (TAI or UTC) | LRO |
| 145987 | FM3003.1 | If the command-specified GetSizeTimeMode flag is set to FALSE, FM shall initialize the following values to Zero:   1. file size in bytes of each file 2. last modification time of each file 3. Mode (permissions), as a 4-byte value, of each file     Note: the lettering of the listed values is kept in sync with parent requirement | Obtaining file size, time, and permissions may be CPU intensive | GPM, NICER |
|  |  | 5.4        Status Reporting |  |  |
| 5570 | FM4000 | FM shall generate a housekeeping message containing the following:   1. Valid Command Counter 2. Command Rejected Counter 3. For each file system: Total number of open files |  | LRO, BAT, JWST |
| 5572 | FM4001 | Upon receipt of a Report Device Free Space command, FM shall generate a message containing for each enabled device in the FM device table the amount of available free space. |  |  |
|  |  | 5.5        Initialization Requirements |  |  |
| 5576 | FM5000 | Upon initialization of the FM Application,   FM shall initialize the following data to Zero:   1. Valid Command Counter 2. Command Rejected Counter | No information is preserved across an FM initialization.  Note that the file system is preserved by the cFE across a processor reset. | LRO, BAT, JWST |

<MKSID-5353>

<MKSID-5361>

 <MKSID-5367>

<MKSID-5369>

<MKSID-5381>

<MKSID-5383>

<MKSID-5385>

<MKSID-5387>

<MKSID-5391>

<MKSID-5393>

<MKSID-5395>

<MKSID-5397>

<MKSID-5399>

<MKSID-5401>

<MKSID-5403>

<MKSID-5405>

<MKSID-5407>

<MKSID-5409>

<MKSID-5411>

<MKSID-5415>

<MKSID-5417>

<MKSID-5427>

<MKSID-5431>

<MKSID-5433>